#!/bin/bash

# Adjust brightness on the most likely display device.
# Usage: nomarchy-brightness-display <step>

step="${1:-+5%}"

# Start with the first possible output, then refine to the most likely given an order heuristic.
device="$(ls -1 /sys/class/backlight 2>/dev/null | head -n1)"
for candidate in amdgpu_bl* intel_backlight acpi_video*; do
  if [[ -e /sys/class/backlight/$candidate ]]; then
    device="$candidate"
    break
  fi
done

# Set the actual brightness of the display device.
brightnessctl -d "$device" set "$step" >/dev/null

# Use SwayOSD to display the new brightness setting.
nomarchy-swayosd-brightness "$(brightnessctl -d "$device" -m | cut -d',' -f4 | tr -d '%')"
